

in front of this big tree is Salohy school





Lining or Cleaning



Successive layers of soils

Main or dominant layer is clay but at 16 000mm till 16 500mm, there, we found a layer which is completely productive.

As it is shown above, during Vohipeno was in a problem of water, five and half months without rain water, Salohy was not touched. It was also built during no water but I’m completely satisfied of it. Really helpful, they are coming out of the problems, dirty water, salty and luck and cause bellyache.



  

  

Entrance or front Rear fence intercepting ditch to protect hand pump





Teaching responsible villagers



North view or left view



south view



East view or Posterior



Fetcher